


**Door Measuring Sheet**

****

*Overall wall to wall door size*

*Measured from the outside*

Smallest Width = \_\_\_\_\_\_mm – Minus 5mm = Final Order Width for Door\_\_\_\_\_\_mm

Smallest Height = \_\_\_\_\_\_mm – Minus 5mm = Final Order Height for Door\_\_\_\_\_\_mm

Summary Guide

More info and video on our website www.diydoubleglazingperth.com.au

* Measure your doors from the outside of the property
* Measure the brickwork/render openings in 3 places for both width and height
* Of the 3 measurements, use the smallest and deduct 5mm,that is your order size